|  |  |
| --- | --- |
| ***Please complete and email to:***  **nexansdrumreturn@mainfreight.co.nz** | **15-98-601** |

Drum Return Acknowledgement

Customer:

Contact Name: Phone:

Email: Date:

Pick Up Address:

Special Instructions:

|  |
| --- |
|  |

**Drum Sizes to be Collected**

|  |  |
| --- | --- |
| **Item and Size** | **Qty** |
| 1 metre Drum |  |
| 1 – 1.6m Drum |  |
| 1.6 – 2.5m Drum |  |
| Pallets |  |
| 350mm Plastic Drum |  |
| WIMA Stillage |  |

**Conditions**

a) Only Nexans items will be accepted.

b) Check for rot, splits, cracks and broken flanges, especially where the drum may have been sitting for a long time on the ground in one place - even a small piece of rot on the flange is no good.

c) Check barrel. Make sure reel core is in good condition *(no rot, not broken or split)*.

**pick-up drivers**: Drums not up to standard are not to be uplifted.